HTC Desire S Rootolása

BEST!!!

http://forum.xda-developers.com/showthread.php?t=1318919

RUU_Saga_HTC_Europe_1.28.401.1_Radio_20.28b.30.0805U_38.03.02.11_M_release_177977_signed.exe

http://www.androidruu.com/index.php?developer=Saga

http://forum.xda-developers.com/showthread.php?t=1146601

http://cmw.cmfs.me/saga/

http://forum.xda-developers.com/showthread.php?t=1146601

A telefon vissza lesz állítva gyári beállításokra

Előfeltételek

HTC-s FastBoot kikapcsolása

USB Debug üzemmód bekapcsolása

HTC Developer portalos felhasználó

HBOOT S-OFF

HBOOT S-OFF megszüntetése, hogy írható legyen a BOOT és HBOOT partíció

Belépés a bootloaderbe:

Kikapcsolt állapotból: VolumeDown+Power

Bekacsolt állapotból:

adb reboot-bootloader

Készülék azonosító lekérdezése:

fastboot oem get_identifier_token #< waiting for device > #... #(bootloader) #(bootloader) < Please cut following message > #(bootloader) <<<< Identifier Token Start >>>> #(bootloader) ... #(bootloader) ... #(bootloader) ... #(bootloader) <<<<< Identifier Token End >>>>> #OKAY [ 0.062s] #finished. total time: 0.062s

Telefon regisztrálása a HTC Developer portálon: http://www.htcdev.com/bootloader/unlock-instructions/

Email-ben kapott feloldó bináris feltöltése:

fastboot flash unlocktoken Unlock_code.bin #sending 'unlocktoken' (0 KB)... #OKAY [ 0.015s] #writing 'unlocktoken'... #(bootloader) unlock token check successfully #OKAY [ 0.005s] #finished. total time: 0.021s

Művelet megerősítése a VolumeUp, majd a Power gombbal!

A telefon újraindul a gyári beállításokra visszaállva

Temp root jogosultság szerzése

http://forum.xda-developers.com/showthread.php?t=1443636

TacoRoot telepítése:

adb push -p tacoroot.bin /data/local/tmp/tacoroot adb shell chmod 777 /data/local/tmp/* /data/local/tmp/tacoroot --setup

Ha a piros felkiáltójel megjelenik, akkor a VolumeUp+VolumeDown+Power gombokkal indítsuk újra a telefont. Olyan hosszan kell nyomni, mintha 2x bootolna, utána lehet csak elengedni. Ezt követően várjuk meg, hogy teljesen betöltsön.

Temp root utolsó lépése:

adb shell /data/local/tmp/tacoroot --root

HBoot downgradelése

http://forum.xda-developers.com/showthread.php?t=1113820

Jelenlegi HBOOT lementése:

adb shell dd if=/dev/block/mmcblk0p18 of=/data/local/tmp/backup.img exit adb pull -p /data/local/tmp/backup.img

Új flashelése:

adb push -p hboot.img /data/local/tmp adb shell chmod 777 /data/local/tmp/hboot.img dd if=/data/local/tmp/hboot.img of=/dev/block/mmcblk0p18

Reboot a boot menübe:

adb reboot-bootloader
fastboot devices //Verify that the device is detected fastboot erase cache //Not sure if this is completely necessary, but the guide I followed included it as a step fastboot oem rebootRUU //Boot into RUU, which lets you flash HBOOT, radio, etc. fastboot flash zip [zipname.zip] //Replace zipname.zip with the actual name of the file you are flashing fastboot reboot-bootloader //The guide I pulled this info from didn't specifically say that you should reboot t

@echo off cls adb devices echo If your device is not listed exit this program now, enable usb debugging and try again. pause cls adb push -p hboot.img /data/local/tmp adb shell chmod 777 /data/local/tmp/hboot.img echo Please accept superuser request on your phone adb shell su pause adb shell dd if=/dev/block/mmcblk0p18 of=/sdcard/backup.img adb shell dd if=/data/local/tmp/hboot.img of=/dev/block/mmcblk0p18 echo Bootloader should be flashed to your device now, backup from old bootloader is saved at /sdcard/backup.img pause adb reboot bootloader

D:\Batyu\bbalazs>adb push -p goldcard /data/local/tmp/ adb server is out of date. killing... * daemon started successfully * 1174 KB/s (19240 bytes in 0.016s) D:\Batyu\bbalazs>adb shell chmod 777 /data/local/tmp/goldcard D:\Batyu\bbalazs>adb shell cat /sys/class/mmc_host/mmc2/mmc2:*/cid > tcid D:\Batyu\bbalazs>cat tcid A megadott nevet (cat) a rendszer nem ismeri fel belső vagy külső parancsként, futtatható programként vagy kötegfájlként. D:\Batyu\bbalazs>type tcid 03534453553038478003b5890c00b8da D:\Batyu\bbalazs>set/p cid= < tcid D:\Batyu\bbalazs>del tcid D:\Batyu\bbalazs>adb shell /data/local/tmp/goldcard -c %cid% -o /data/local/tmp/goldcard.img HTC android goldcard tool Copyright (C) 2011, Wayne D. Hoxsie Jr. Original code by B. Kerler. Special thanks to ATTN1 and the XDA team. Donations can be made to the Electronic Frontier Foundation: http://www.eff.org/ or to B. Kerler: http://psas.revskills.de/ D:\Batyu\bbalazs>adb shell dd if=/data/local/tmp/goldcard.img of=/dev/block/mmcblk1 /dev/block/mmcblk1: cannot open for write: Permission denied D:\Batyu\bbalazs>adb shell dd if=/data/local/tmp/goldcard.img of=/dev/block/mmcblk D:\Batyu\bbalazs>ls -al /dev/block A megadott nevet (ls) a rendszer nem ismeri fel belső vagy külső parancsként, futtatható programként vagy kötegfájlként. D:\Batyu\bbalazs>adb shell ls -al /dev/block -al: No such file or directory mmcblk1p1 mmcblk1 mmcblk0p31 mmcblk0p30 mmcblk0p29 mmcblk0p28 mmcblk0p27 mmcblk0p26 mmcblk0p25 mmcblk0p24 mmcblk0p23 mmcblk0p22 mmcblk0p21 mmcblk0p20 mmcblk0p19 mmcblk0p18 mmcblk0p17 mmcblk0p16 mmcblk0p15 mmcblk0p14 mmcblk0p13 mmcblk0p12 mmcblk0p11 mmcblk0p10 mmcblk0p9 mmcblk0p8 mmcblk0p7 mmcblk0p6 mmcblk0p5 mmcblk0p4 mmcblk0p3 mmcblk0p2 mmcblk0p1 mmcblk0 loop7 loop6 loop5 loop4 loop3 loop2 loop1 loop0 vold platform D:\Batyu\bbalazs>adb shell su # ^C D:\Batyu\bbalazs>fdish A megadott nevet (fdish) a rendszer nem ismeri fel belső vagy külső parancsként, futtatható programként vagy kötegfájlként. D:\Batyu\bbalazs>fdis D:\Batyu\bbalazs>adb shell $ su su # fdisk fdisk BusyBox v1.19.3 (2011-11-22 01:37:10 MST) multi-call binary. Usage: fdisk [-ul] [-C CYLINDERS] [-H HEADS] [-S SECTORS] [-b SSZ] DISK Change partition table -u Start and End are in sectors (instead of cylinders) -l Show partition table for each DISK, then exit -b 2048 (for certain MO disks) use 2048-byte sectors -C CYLINDERS Set number of cylinders/heads/sectors -H HEADS -S SECTORS # fdisk -^C D:\Batyu\bbalazs>adb shell $ su su # adb shell dd if=/data/local/tmp/goldcard.img of=/dev/block/mmcblk1 # adb shell dd if=/data/local/tmp/goldcard.img of=/dev/block/mmcblk1 adb: not found # # # fdisk /dev/block/mmcblk1 fdisk /dev/block/mmcblk1 The number of cylinders for this disk is set to 19165. There is nothing wrong with that, but this is larger than 1024, and could in certain setups cause problems with: 1) software that runs at boot time (e.g., old versions of LILO) 2) booting and partitioning software from other OSs (e.g., DOS FDISK, OS/2 FDISK) Command (m for help): p p Disk /dev/block/mmcblk1: 7948 MB, 7948206080 bytes 81 heads, 10 sectors/track, 19165 cylinders Units = cylinders of 810 * 512 = 414720 bytes Device Boot Start End Blocks Id System /dev/block/mmcblk1p1 11 19166 7757824 b Win95 FAT32 Command (m for help): q q # shell dd if=/data/local/tmp/goldcard.img of=/dev/block/mmcblk1 shell dd if=/data/local/tmp/goldcard.img of=/dev/block/mmcblk1 shell: not found # dd if=/data/local/tmp/goldcard.img of=/dev/block/mmcblk1 dd if=/data/local/tmp/goldcard.img of=/dev/block/mmcblk1 0+1 records in 0+1 records out 384 bytes transferred in 0.001 secs (384000 bytes/sec) # ^C D:\Batyu\bbalazs>adb reboot D:\Batyu\bbalazs>adb shell $ su su # /data/local/tmp/misc_version -s 1.27.405.6 /data/local/tmp/misc_version -s 1.27.405.6 --set_version set. VERSION will be changed to: 1.27.405.6 Patching and backing up misc partition... # exit exit $ adb reboot-bootloader adb reboot-bootloader adb: permission denied $ ^Cb reboot-bootloader D:\Batyu\bbalazs>^D D:\Batyu\bbalazs>adb reboot-bootloader D:\Batyu\bbalazs>fastboot oem lock ... (bootloader) Lock successfully... FAILED (status read failed (Too many links)) finished. total time: 0.301s D:\Batyu\bbalazs>adb reboot-bootloader D:\Batyu\bbalazs>