Phoscon - ConBee2

deConz telepítése Ubuntu-n

https://phoscon.de/en/conbee2/install#ubuntu

Ha a deConz nem látja az USB-Gatewayt, fel kell frissíteni legalább 2.05.65-es verzióra.
A dialout csoportba való felvétel után újra be kell jelenzkezni a felhasználóval, hogy érvénybe lépjen a csoporttagságunk.

dmesg hiba

cdc_acm 1-2:1.0: failed to set dtr/rts:

usb 1-2: new full-speed USB device number 31 using xhci_hcd
usb 1-2: New USB device found, idVendor=1cf1, idProduct=0030
usb 1-2: New USB device strings: Mfr=1, Product=2, SerialNumber=3
usb 1-2: Product: ConBee II
usb 1-2: Manufacturer: dresden elektronik ingenieurtechnik GmbH
usb 1-2: SerialNumber: DE1997960
cdc_acm 1-2:1.0: ttyACM0: USB ACM device
usb 1-2: USB disconnect, device number 31
cdc_acm 1-2:1.0: failed to set dtr/rts
usb 1-2: new full-speed USB device number 32 using xhci_hcd
usb 1-2: New USB device found, idVendor=1cf1, idProduct=0030
usb 1-2: New USB device strings: Mfr=1, Product=2, SerialNumber=3
usb 1-2: Product: ConBee II
usb 1-2: Manufacturer: dresden elektronik ingenieurtechnik GmbH
usb 1-2: SerialNumber: DE1997960
cdc_acm 1-2:1.0: ttyACM0: USB ACM device

Kell egy /etc/udev/rules.d/10-dresden-conbee-ii.rules szabály :

ATTRS{idVendor}=="1d6b", ATTRS{idProduct}=="0002", ENV{ID_MM_DEVICE_IGNORE}="1" ATTRS{idVendor}=="1d6b", ATTRS{idProduct}=="0002", ENV{MTP_NO_PROBE}="1" SUBSYSTEMS=="usb", ATTRS{idVendor}=="1d6b", ATTRS{idProduct}=="0002", MODE:="0666" KERNEL=="ttyACM*", ATTRS{idVendor}=="1d6b", ATTRS{idProduct}=="0002", MODE:="0666"