UniFi SSH

Command	Example	Function
info	info	Displays device information
set-default	set-default	Factory reset device
set-inform	set-inform http://192.168.1.1:8080/inform	Set URL of the controller for adoption. More info
upgrade	upgrade https://<firmware-url>.bin	Upgrade firmware – More info
fwupdate	fwupdate --url https://<firmware-url>.bin	Update firmware
reboot	reboot	Reboot the device
poweroff	poweroff	Shutdown device
uptime	uptime	Shows device uptime

lazyadmin.nl