UPS

https://www.muszeroldal.hu/assistance/fogalomtar.pdf

Jelalakok

https://www.quora.com/Is-a-200W-power-inverter-a-pure-sine-wave-inverter

Négyszögjel

„Square wave”

Lépcsős színusz

„Stepped Sine wave”

„Stepped approximation to a sinewave” = „Lépésenkénti közelítés egy szinuszhullámhoz”

pl. az APC Back-UPS és APC Easy-UPS termékcsaládok
Az Easy nem rendelkezik USB kapcsolattal.

Tiszta színusz

„Sine wave”

„Pure Sine Wave”

pl. az APC Smart-UPS termékcsalád (750VA fölött)
Egyelőre nem teljesen világos, hogy mi a különbség az APC Smart-UPS SMC („Pure Sine Wave”) és SMT („Sine wave”) jelalakjai között. (egy doksi)

Topológiák

http://www.bitronix.hu/milyen_szunetmentest

Offline

„Standby” = „Készenlét”

Vonal-interaktív

„Line-interactive”

Online

„Double Conversion Online” = „Online - dupla konverzió”

Csúcsfeszültség-faktor

Understanding Power Factor, Crest Factor, and Surge Factor

http://azimadli.com/vibman/crestfactor1.htm

crest factor

crest factor = |peak current| / rms current

crest factor = |peak current| / rms current = 7.07 A / 5 A = 1.414

crest factor = |peak current| / rms current = 21.21 A / 5 A = 4.24

Why is crest factor important?

spec http://blog.powerandtest.com/blog/what-is-crest-factor-and-why-is-it-important